IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView, QuantityTakeOffAddOnView]"
File name: "Projektnummer"
Time stamp: "2017-02-22T11:19:14"
Preprocessor: "The EXPRESS Data Manager Version 5.01.0100.02.64mod : 6 Jun 2012"
Originating system: "20130308_1515(x64) - Exporter 2014.0.2013.0308 - Default UI"
Application: "Autodesk Revit 2014 (DEU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (DEU)"

People and organizations
  Person "Mklein" of Organization (no name given)
  Owner history of Person "Mklein" of Organization (no name given) | application "Autodesk Revit 2014 (DEU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (DEU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: KELVIN
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  POWERUNIT: WATT

Spatial structure
IFCPROJECT "Projektnummer" | long name "Projektname" | phase "Projektstatus"
  IFCSITE "Default" | latitude 48° 8′ 20.852966″ | longitude 11° 34′ 48.669204″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Projektadresse", "München", "Deutschland"
      IFCBUILDINGSTOREY "Ebene 0" | long name "Ebene 0" | elevation 0.
        contains 6 elements
          1 x IFCBUILDINGELEMENTPROXY | object type "calorSchwank D 15 U" | names: "Heater-Schwank_GmbH-Tube_Heaters-calorSchwank_U__02_2017:calorSchwank D 15 U:332241" | material: materials ("Paint - Schwank - Flaked Reflective - Beige", "Plastic - Schwank - Coarse Textured - Dark Gray", "Plastic - Schwank - Low Gloss - Black", "Plastic- Schwank - Smooth") | property sets: Sonstige, HLS, Abmessungen, Abhängigkeiten, Elektro - Lasten, Phasen
          1 x IFCBUILDINGELEMENTPROXY | object type "calorSchwank D 20 U" | names: "Heater-Schwank_GmbH-Tube_Heaters-calorSchwank_U__02_2017:calorSchwank D 20 U:332253" | material: materials ("Paint - Schwank - Flaked Reflective - Beige", "Plastic - Schwank - Coarse Textured - Dark Gray", "Plastic - Schwank - Low Gloss - Black", "Plastic- Schwank - Smooth") | property sets: HLS, Sonstige, Phasen, Abhängigkeiten, ID-Daten, Abmessungen
          1 x IFCBUILDINGELEMENTPROXY | object type "calorSchwank D 30 U" | names: "Heater-Schwank_GmbH-Tube_Heaters-calorSchwank_U__02_2017:calorSchwank D 30 U:332265" | material: materials ("Paint - Schwank - Flaked Reflective - Beige", "Plastic - Schwank - Coarse Textured - Dark Gray", "Plastic - Schwank - Low Gloss - Black", "Plastic- Schwank - Smooth") | property sets: HLS, Abhängigkeiten, Abmessungen, Elektro - Lasten, Sonstige, Phasen
          1 x IFCBUILDINGELEMENTPROXY | object type "calorSchwank D 40 U" | names: "Heater-Schwank_GmbH-Tube_Heaters-calorSchwank_U__02_2017:calorSchwank D 40 U:332277" | material: materials ("Paint - Schwank - Flaked Reflective - Beige", "Plastic - Schwank - Coarse Textured - Dark Gray", "Plastic - Schwank - Low Gloss - Black", "Plastic- Schwank - Smooth") | property sets: Abhängigkeiten, Sonstige, HLS, Phasen, ID-Daten, Elektro - Lasten
          1 x IFCBUILDINGELEMENTPROXY | object type "calorSchwank D 50 U" | names: "Heater-Schwank_GmbH-Tube_Heaters-calorSchwank_U__02_2017:calorSchwank D 50 U:332292" | material: materials ("Paint - Schwank - Flaked Reflective - Beige", "Plastic - Schwank - Coarse Textured - Dark Gray", "Plastic - Schwank - Low Gloss - Black", "Plastic- Schwank - Smooth") | property sets: Abhängigkeiten, Abmessungen, HLS, Sonstige, ID-Daten, Phasen
          1 x IFCBUILDINGELEMENTPROXY | object type "calorSchwank D 60 U" | names: "Heater-Schwank_GmbH-Tube_Heaters-calorSchwank_U__02_2017:calorSchwank D 60 U:332307" | material: materials ("Paint - Schwank - Flaked Reflective - Beige", "Plastic - Schwank - Coarse Textured - Dark Gray", "Plastic - Schwank - Low Gloss - Black", "Plastic- Schwank - Smooth") | property sets: HLS-Volumenstrom, Eigenschaften für ökologisches Bauen, Elektro, Abhängigkeiten, Materialien und Oberflächen, Konstruktion

Property sets
  Abhängigkeiten | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Basisbauteil = "Ebene : Ebene 0" (IFCTEXT)
    Bottom Clearance to Combustibles = 1.1 (IFCLENGTHMEASURE) [METRE]
    Burner Side Clearance to Combustibles = 0.15 (IFCLENGTHMEASURE) [METRE]
    Ebene = "Ebene: Ebene 0" (IFCLABEL)
    Flue Gas Clearance to Combustibles = 0.35 (IFCLENGTHMEASURE) [METRE]
    Top Clearance to Combustibles = 0.5 (IFCLENGTHMEASURE) [METRE]
    Versatz = 0. (IFCLENGTHMEASURE) [METRE]
  Abhängigkeiten | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Front Clearance to Combustibles = 0.1 (IFCLENGTHMEASURE) [METRE]
  Abhängigkeiten | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Basishöhe = "Projekt-Basispunkt" (IFCIDENTIFIER)
  Abhängigkeiten | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Ansicht = 0. (IFCLENGTHMEASURE) [METRE]
  Grafiken | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Farbe = 16711680 (IFCINTEGER)
    Linienmuster = "Verdeckt" (IFCLABEL)
    Linienstärke = "1" (IFCIDENTIFIER)
    Symbol = "Beschriftung Ebene: Beschriftung Ebene" (IFCLABEL)
    Symbol bei Ende 1 Standard = FALSE (IFCBOOLEAN)
    Symbol bei Ende 2 Standard = TRUE (IFCBOOLEAN)
  HLS-Volumenstrom | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Eigenschaften für ökologisches Bauen | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    ecoScorecard Product Page = "http://ecoscorecard.com/" (IFCTEXT)
  Sonstige | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Angle Control = 20. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Edit Formula Control = TRUE (IFCBOOLEAN)
  Sonstige | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Base = FALSE (IFCBOOLEAN)
    Dimension A = 0.1 (IFCLENGTHMEASURE) [METRE]
    Dimension B = 0.15 (IFCLENGTHMEASURE) [METRE]
    Dimension C = 1.1 (IFCLENGTHMEASURE) [METRE]
    Dimension D = 0.35 (IFCLENGTHMEASURE) [METRE]
    Dimension E = 0.5 (IFCLENGTHMEASURE) [METRE]
    Dimension F = 0.15 (IFCLENGTHMEASURE) [METRE]
    Dimension G = 1.1 (IFCLENGTHMEASURE) [METRE]
    Dimension H = 0.35 (IFCLENGTHMEASURE) [METRE]
  Sonstige | properties | on 1 object (1 IFCBUILDING)
    Kundenname = "Bauherr" (IFCTEXT)
    Projektadresse = "Projektadresse" (IFCTEXT)
    Projektausgabedatum = "Projekt Datum" (IFCTEXT)
    Projektname = "Projektname" (IFCTEXT)
    Projektnummer = "Projektnummer" (IFCTEXT)
    Projektstatus = "Projektstatus" (IFCTEXT)
    Verfasser Firma 1 = "Firma 1" (IFCTEXT)
    Verfasser Firma 2 = "Firma 2" (IFCTEXT)
    Verfasser PLZ Ort = "PLZ Ort" (IFCTEXT)
    Verfasser Strasse = "Strasse" (IFCTEXT)
    Verfasser Telefax = "Telefax" (IFCTEXT)
    Verfasser Telefon = "Telefon" (IFCTEXT)
    Verfasser eMail = "E-Mail" (IFCTEXT)
  HLS | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Gas Pressure Line Minimum = 457.2 (IFCREAL)
    Liquid Propane = FALSE (IFCBOOLEAN)
    Natural Gas = TRUE (IFCBOOLEAN)
    Systemklassifizierung = "Sonstige,Energie,Abluft 2" (IFCTEXT)
    Systemname = "" (IFCTEXT)
  HLS | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Gas Flow Rate = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Gas Inlet Radius = 0.00635 (IFCLENGTHMEASURE) [METRE]
    Gas Pressure Line Maximum = 1828.8 (IFCREAL)
    IR Output = 11400. (IFCPOWERMEASURE) [WATT]
    Radiant Efficiency = "65.3%" (IFCTEXT)
    Rating Natural Gas = 14999.9986820831 (IFCPOWERMEASURE) [WATT]
    Thermal Efficiency = "94%" (IFCTEXT)
  Abmessungen | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Angle = 20. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Minimum Mounting Height = 3.1 (IFCLENGTHMEASURE) [METRE]
  Abmessungen | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Höhe für Berechnung = 0. (IFCLENGTHMEASURE) [METRE]
  Abmessungen | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Exhaust Radius = 0.05 (IFCLENGTHMEASURE) [METRE]
    Heater Box Length = 0.445 (IFCLENGTHMEASURE) [METRE]
    Height = 0.315 (IFCLENGTHMEASURE) [METRE]
    Overall Length with Controls = 3.582 (IFCLENGTHMEASURE) [METRE]
    Width = 0.584 (IFCLENGTHMEASURE) [METRE]
  Abmessungen | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Exhaust Radius = 0.05 (IFCLENGTHMEASURE) [METRE]
    Heater Box Length = 0.445 (IFCLENGTHMEASURE) [METRE]
    Height = 0.315 (IFCLENGTHMEASURE) [METRE]
    Overall Length with Controls = 5.072 (IFCLENGTHMEASURE) [METRE]
    Width = 0.584 (IFCLENGTHMEASURE) [METRE]
  Abmessungen | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Exhaust Radius = 0.05 (IFCLENGTHMEASURE) [METRE]
    Heater Box Length = 0.445 (IFCLENGTHMEASURE) [METRE]
    Height = 0.315 (IFCLENGTHMEASURE) [METRE]
    Overall Length with Controls = 6.632 (IFCLENGTHMEASURE) [METRE]
    Width = 0.584 (IFCLENGTHMEASURE) [METRE]
  Abmessungen | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Exhaust Radius = 0.05 (IFCLENGTHMEASURE) [METRE]
    Heater Box Length = 0.47 (IFCLENGTHMEASURE) [METRE]
    Height = 0.315 (IFCLENGTHMEASURE) [METRE]
    Overall Length with Controls = 9.558 (IFCLENGTHMEASURE) [METRE]
    Width = 0.584 (IFCLENGTHMEASURE) [METRE]
  Abmessungen | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Exhaust Radius = 0.05 (IFCLENGTHMEASURE) [METRE]
    Heater Box Length = 0.47 (IFCLENGTHMEASURE) [METRE]
    Height = 0.315 (IFCLENGTHMEASURE) [METRE]
    Overall Length with Controls = 12.608 (IFCLENGTHMEASURE) [METRE]
    Width = 0.584 (IFCLENGTHMEASURE) [METRE]
  Abmessungen | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Exhaust Radius = 0.05 (IFCLENGTHMEASURE) [METRE]
    Heater Box Length = 0.47 (IFCLENGTHMEASURE) [METRE]
    Height = 0.315 (IFCLENGTHMEASURE) [METRE]
    Overall Length with Controls = 14.098 (IFCLENGTHMEASURE) [METRE]
    Width = 0.584 (IFCLENGTHMEASURE) [METRE]
  Elektro - Lasten | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Element = "" (IFCTEXT)
    Stromkreisnummer = "" (IFCTEXT)
  Elektro - Lasten | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Apparent Load = 0. (IFCREAL)
    Load Classification = "Power" (IFCLABEL)
    Load Sub Classification Motor = FALSE (IFCBOOLEAN)
    Power Factor = 1. (IFCREAL)
  Phasen | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Phase erstellt = "Phase 1" (IFCLABEL)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Kennzeichen = "1" (IFCTEXT)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Kennzeichen = "2" (IFCTEXT)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Kennzeichen = "3" (IFCTEXT)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Kennzeichen = "4" (IFCTEXT)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Kennzeichen = "5" (IFCTEXT)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Kennzeichen = "6" (IFCTEXT)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Gebäudegeschoss = TRUE (IFCBOOLEAN)
    Name = "Ebene 0" (IFCTEXT)
    Tragwerk = FALSE (IFCBOOLEAN)
  ID-Daten | properties | on 1 object (1 IFCBUILDING)
    Autor = "" (IFCTEXT)
    Beschreibung von Unternehmen = "" (IFCTEXT)
    Gebäudename = "" (IFCTEXT)
    Unternehmensname = "" (IFCTEXT)
  ID-Daten: 6 more contents on 6 objects not shown
  Pset_ManufacturerTypeInformation | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "Schwank GmbH" (IFCLABEL)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "calorSchwank D 15 U" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "calorSchwank D 20 U" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "calorSchwank D 30 U" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "calorSchwank D 40 U" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "calorSchwank D 50 U" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "calorSchwank D 60 U" (IFCIDENTIFIER)
  Elektro | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Electrical Supply Amperage = 0. (IFCREAL)
    Electrical Supply Frequency = 50. (IFCREAL)
    Electrical Supply Voltage = 2475.69939584324 (IFCREAL)
    Number of Poles = 1 (IFCINTEGER)
  Materialien und Oberflächen | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Heater = "Matal - Schwank - Copper - Satin Brushed" (IFCLABEL)
    Unit = "Matal - Schwank - Semi - Polished" (IFCLABEL)
  Konstruktion | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Exhaust Air Connector = "Exhaust Air Connector" (IFCTEXT)
    Gas Inlet Connector = "Gas Inlet Connection" (IFCTEXT)
    Power Connector = "Power Connection" (IFCTEXT)
  Text | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Brochure URL = "" (IFCTEXT)
    Manual URL = "" (IFCTEXT)
    Technical Information = "" (IFCTEXT)
    Warranty URL = "" (IFCTEXT)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)