IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView, QuantityTakeOffAddOnView]"
Time stamp: "2017-02-22T12:34:47"
Preprocessor: "The EXPRESS Data Manager Version 5.01.0100.02.64mod : 6 Jun 2012"
Originating system: "20130308_1515(x64) - Exporter 2014.0.2013.0308 - Default UI"
Application: "Autodesk Revit 2014 (DEU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (DEU)"

People and organizations
  Person "Mklein" of Organization (no name given)
  Owner history of Person "Mklein" of Organization (no name given) | application "Autodesk Revit 2014 (DEU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (DEU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: KELVIN
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  POWERUNIT: WATT

Spatial structure
IFCPROJECT | long name "P:\1Hallen\Klein M__Revit\primo\Projekt34.ifc"
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Ebene 1" | long name "Ebene 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | object type "primoSchwank-40" | names: "Space_Heater-Schwank-High_Intensity-primoSchwank-40:primoSchwank-40:5830" | material: materials ("Matal - Schwank - Semi - Polished", "Matal - Schwank - Copper - Satin Brushed") | property sets: Phasen, ID-Daten, Abhängigkeiten, HLS, Elektro - Lasten, Pset_ManufacturerTypeInformation

Property sets
  Abhängigkeiten | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Basishöhe = "Projekt-Basispunkt" (IFCIDENTIFIER)
  Abhängigkeiten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Basisbauteil = "Ebene : Ebene 1" (IFCTEXT)
    Ebene = "Ebene: Ebene 1" (IFCLABEL)
    Versatz = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Abhängigkeiten | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Ansicht = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Abhängigkeiten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Bottom Clearance to Combustibles = "Dimension G" (IFCTEXT)
    Front Clearance to Combustibles = "Dimension D" (IFCTEXT)
    Rear Clearance to Combustibles = "Dimension F" (IFCTEXT)
    Top Clearance to Combustibles = "Dimension E" (IFCTEXT)
  Phasen | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase erstellt = "Neue Konstruktion" (IFCLABEL)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Kennzeichen = "1" (IFCTEXT)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Gebäudegeschoss = TRUE (IFCBOOLEAN)
    Name = "Ebene 1" (IFCTEXT)
    Tragwerk = FALSE (IFCBOOLEAN)
  ID-Daten | properties | on 1 object (1 IFCBUILDING)
    Beschreibung von Unternehmen = "" (IFCTEXT)
    Gebäudename = "" (IFCTEXT)
    Unternehmensname = "" (IFCTEXT)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    04 CSI = "23 83 33" (IFCTEXT)
    95 CSI = "15768" (IFCTEXT)
    Baugruppenbeschreibung = "Heat Generating Systems" (IFCTEXT)
    Baugruppenkennzeichen = "D3020" (IFCTEXT)
    Beschreibung = "High Intensity Heaters, primoSchwank- 40" (IFCTEXT)
    Cost Info = "mailto:csr@schwankgroup.com" (IFCTEXT)
    Hersteller = "Schwank" (IFCTEXT)
    Manufacturer Address = "2 Schwank Way, Waynesboro, GA 30830" (IFCTEXT)
    Manufacturer Email = "mailto:csr@schwankgroup.com" (IFCTEXT)
    Manufacturer Fax = "1-866-724-9265" (IFCTEXT)
    Manufacturer Phone - Toll Free = "1-877-446-3727" (IFCTEXT)
    Manufacturer Phone = "1-877-446-3727" (IFCTEXT)
    Modell = "primoSchwank- 40" (IFCTEXT)
    OmniClass-Nummer = "23.75.10.17.14.14" (IFCTEXT)
    OmniClass-Titel = "Fuel-Fired Radiant Heaters" (IFCTEXT)
    Product Page URL = "http://www.schwankusa.com/high-intensity-heaters/primo/" (IFCTEXT)
    Subcategory = "High Intensity Heaters" (IFCTEXT)
    URL = "http://www.schwankusa.com" (IFCTEXT)
    Weight = 1152.9183320393 (IFCREAL)
    ecoScorecard_data = "" (IFCTEXT)
  HLS | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Systemklassifizierung = "Energie,Sonstige" (IFCTEXT)
    Systemname = "" (IFCTEXT)
  HLS | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Gas Inlet Radius = 6.35 (IFCLENGTHMEASURE) [MILLI METRE]
    Gas Pressure Line WC Maximum = "14" (IFCTEXT)
    Gas Pressure Line WC Minimum = "6" (IFCTEXT)
    Gas Pressure WC Manifold = "5" (IFCTEXT)
    IR Output = 28603.7364488089 (IFCPOWERMEASURE) [WATT]
    Liquid Propane = FALSE (IFCBOOLEAN)
    Natural Gas = TRUE (IFCBOOLEAN)
    Radiant Efficiency = "65.10%" (IFCTEXT)
    Rating Natural Gas = 43960.6605258333 (IFCPOWERMEASURE) [WATT]
    Thermal Efficiency = ">85%" (IFCTEXT)
  Elektro - Lasten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Element = "" (IFCTEXT)
    Stromkreisnummer = "" (IFCTEXT)
  Elektro - Lasten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Apparent Load = 0. (IFCREAL)
    Load Classification = "Power" (IFCLABEL)
    Load Sub Classification Motor = FALSE (IFCBOOLEAN)
    Number of Poles = 1 (IFCINTEGER)
    Power Factor = 1. (IFCREAL)
    Voltage = 0. (IFCREAL)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "Schwank" (IFCLABEL)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "primoSchwank-40" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Abmessungen | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Höhe für Berechnung = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Abmessungen | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Angle = 30. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Heater Box Length = 1158.748 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 295.275 (IFCLENGTHMEASURE) [MILLI METRE]
    Minimum Mounting Height = 8534.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Length with Controls = 1412.748 (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 762. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Sonstige | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Angle Control = 30. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Base = FALSE (IFCBOOLEAN)
    Box Width C = 1147.318 (IFCLENGTHMEASURE) [MILLI METRE]
    Dimension A = 660.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Dimension B = 1143. (IFCLENGTHMEASURE) [MILLI METRE]
    Dimension C = 2794. (IFCLENGTHMEASURE) [MILLI METRE]
    Dimension D = 203.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Dimension E = 1219.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Dimension F = 1981.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Dimension G = 914.4 (IFCLENGTHMEASURE) [MILLI METRE]
  Materialien und Oberflächen | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Heater = "Matal - Schwank - Copper - Satin Brushed" (IFCLABEL)
    Unit = "Matal - Schwank - Semi - Polished" (IFCLABEL)
  Elektro | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Control Amperage = 0.55 (IFCREAL)
    Control Frequency = 60. (IFCREAL)
    Control Voltage = 258.333850001033 (IFCREAL)
  Text | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Brochure URL = "http://www.schwankusa.com/fileadmin/pdf/Schwank%20Literature/Product_Brochures/primoSchwank%20October%2024.pdf" (IFCTEXT)
    Manual URL = "http://www.schwankusa.com/fileadmin/pdf/Manuals/High_Intensity_Heaters/supra_primo_Manual_12C_NOV-2011.pdf" (IFCTEXT)
    Technical Information = "http://www.schwankusa.com/fileadmin/pdf/Tech_Specs/High_Intensity/primo_Tech_Specs_TS090921_RL-01B.pdf" (IFCTEXT)
    Warranty URL = "http://www.schwankusa.com/fileadmin/pdf/Forms/Schwank_Warranty_Summary_Nov-2012.pdf" (IFCTEXT)
  Konstruktion | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Gas Inlet Connector = "Gas Inlet Connector" (IFCTEXT)
    Power Connector = "Power Connection" (IFCTEXT)
  Eigenschaften für ökologisches Bauen | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    ecoScorecard Product Page = "http://ecoscorecard.com/" (IFCTEXT)
  Grafiken | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Farbe = 0 (IFCINTEGER)
    Linienmuster = "-3000010" (IFCLABEL)
    Linienstärke = "1" (IFCIDENTIFIER)
    Symbol bei Ende 1 Standard = FALSE (IFCBOOLEAN)
    Symbol bei Ende 2 Standard = TRUE (IFCBOOLEAN)